These are notes on how to build and deploy the firmware to Ez, but they are
from before the qmk restructuring.

cd qmk_firmware/keyboard/ergodox_ez
make KEYMAP=jafo
cp ergodox_ez.hex keymaps/jafo/
/tmp/teensy.64bit
Open hex keymap file
Program
Upload
